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Description
Puzzle blends performance, sustainability, and a bold visual language into one striking modular concept. The pendant luminaire features a shadow-free glowing light effect, smart system readiness, and modern aesthetics. 
USP
· Pendant mounting options with driver in canopy for concrete & wooden ceilings and driver on ceiling for false ceilings
· Continuous glowing light effect through transparent body
· Various light recipes: 3000K, 4000K, CRI 90+
· Office compliant
· Heat resistant & impact resistant PET-G material for housing
· Printed with mass-balanced 50% recycled copolyester materials 
· Driver options: PSU (Non Dimming) / DIA (Dali Interact Dimming) / WIA (Wireless Interact dimming) / SIA (Sensor ready driver)
· Interact ready
· Integrated sensor option for presence detection and daylight control
· EPD document available (Environmental Product Declaration)
· Disassembly instructions available
The Projector complies with the following standards:
· [bookmark: _Hlk140587000]CE marked
· RoHS
Specifications: 
· Efficacy up to 152 lm/W
· CRI90, Color temperature: 3000K / 4000K
· Lumen: 4000 and 5000
· Lumen maintenance: 72,000hrs to L80 @ 25°C Ta 
· Driver Failure Rate <1% @ 5,000 hrs
· IP20 / IK02
· Electrical Class II
· Ambient range: +10°C to +35°C
· Glow wire test 650°C
· 5-year warranty
· Binning: CRI90 SDCM<2
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Dimensional drawing
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