**JTD 908 / 1109 Update Instructions**

1. Connect the unit to the computer using a RS232 – RS232 cable. \**RS232 – USB cable may not work*
2. Open “COMISP V1.00.02” executable
3. Turn the unit off
4. In the “COMISP V1.00.02” menu, select “COM 1” under “COM select” Option
5. Click on the drop-down menu under “MCU select” and select “LQFP48”
6. Click on “Connect”
7. Click on “Open”, and select the “JTD-908 V2.5-US0056.hex” file
8. Click on “Upgrade”. After clicking on “Upgrade”, turn the unit on
9. The firmware will start updating, and the progress can be viewed via the loading bar in the bottom left corner of the software
10. After the update is complete, close the “COMISP V1.00.02” window
11. Open the controller software “HDMI-944Vv6.27” executable, and click on “Connect”. The unit will now be updated with the latest firmware

\**Numbers in red circle reflect the bullet points in the article*

