P8 for JTD-669

File JTD669.rss: lib for RS232

File JTD-669-IR.irr: lib for IR

File JTD-669-RS232.wpp: only include RS232 command

File JTD-669-IR-RS232.wpp: include both IR and RS232 command

\*Power p8 with Power Cable

\*If you want to use RS232, please connect RS232(2) to the JTD669 device.

( make sure the TX port on the p8 is connected to the RX port on the JTD669 device.)

( make sure the RX port on the p8 is connected to the TX port on the JTD669 device.)

\*If you want to use IR, please connect IR1 to IR cable.

button1：change source of output1

button2：change source of output2

button3：change source of output3

button4：change source of output4

button5：vol/mute control of output1

button6：vol/mute control of output2

button7：vol/mute control of output3

button8：vol/mute control of output4