
First, Copy the “update.bin” to a flash disk.

Then, power on the unit, and connect the unit to a display.

1. Connect the “service” port on the unit to the flash disk via a double female ports USB cable.

2. Simultaneously, press “MODE” and “RESO” buttons for 5 seconds. On the display, there will show firmware version number and “Firmware update…”. Then you can release the hands. After updating successfully, the unit will restart.

(If failed, there will show “Firmware update failed”)



3.After update, you can check the firmware version number. Remove the disk, and simultaneously press “MODE” and “RESO” buttons for 5 seconds. On the display, there will show firmware version number.