SX:ACCESS (EX2) - How to Upgrade Firmware

1. Connect the SX:ACCESS (EX2) to your PC so that the software can connect to it.

2. Start "Flash.exe". It's in this directory.

3. Enter the IP-address for the SX:ACCESS (EX2).

4. Click on "Download" and choose the .bin-file to be used for programming.

5. The programming takes a few seconds, followed by the unit restarting.

6. Done, new firmware loaded.