Vogl

**How to specify VoglFuge® / VoglJoint system**

* Interior panelling to be VoglFuge®/VoglJoint Ceiling System by Decor Systems
* Contact Decor Systems on Ph: 1800 835 035.
* Profile: \_\_\_\_\_(Insert code according to profile chosen and acoustic requirement)
* **Vogl**Fuge®/**Vogl**Joint System should be installed as per manufacturer’s instructions. Acoustic Panel type cannot to be substituted unless agreed by Architect and Acoustic Engineer \_\_\_\_\_\_\_\_\_\_\_\_
* Panels to be ​Fire Group 1 ​per BCA ​Specification ​C1.10 clause 4.
* Vogl cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​50 years.
* **(Please contact Decor Systems for your project specific completion number)**