DecorSlat Max

**How to write your specification:**

* Interior Beams shall be **DecorSlat** Max by Decor Systems.
* Supplier Decor Systems Ph: 1800 835 035
* Depth: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (145 / 195 / 295mm) [You are free to nominate a custom depth and even vary the depths]
* Beams to be installed at \_\_\_\_ centres
* Finish: Veneer/Laminate: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Decor Systems ​engineering ​certification ​to be supplied for ceiling ​fixing system. ​
* Beams to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4 ​  
  [Note that ​fire group 1 is ​only available ​in the ​SmartLook and DecorImage range of finishes type and ​Group 2 in ​Natural Timber Veneers]​
* DecorSlat Max cannot to be substituted unless agreed by Architect and Acoustic Engineer and panels must be supplied with Decor Systems Certificate Number \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Panels should be allowed to acclimatise on site for at least five days before installation.

* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* Installation to ​be done by an ​approved ​ceiling and ​partition ​contractor.​

**(Please contact Decor Systems for your project specific completion number)**