Cewood

**HOW TO WRITE UP YOUR SPECIFICATION**

* Interior panelling shall be **Cewood** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Thickness Panel: \_\_\_\_mm (15/25/35mm)
* Strand Structure to be \_\_\_\_\_\_\_\_\_\_\_ [please choose a thickness strand option:
  + • S — Super Fine, 1 mm
  + • F — Fine, 1.5 mm
  + • R — Regular, 3 mm
* Edge Profile to be \_\_\_\_\_\_\_\_\_\_ please choose an edging option:
  + PO – Panel without Chamfer
  + P5 – Panel with 5mm chamfer
  + P11 – Panel with 11mm chamfer
  + PO-T24 Standard T24 ceiling profile
  + P0G-T24 Immersed Ceiling Profile
  + P5G-T24 – Immersed ceiling profile with 5mm chamfer
  + P5H - Hidden suspended ceiling profile with 5 mm chamfer
  + P5S - Hidden suspended ceiling profile with overhang and 5 mm chamfer
* Panels to be coloured to be \_\_\_\_\_\_ [Natural or RAL \_\_\_\_\_\_\_ (Insert Code)]
* Panels to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4. ​[Note that fire ​groups 1 is ​only available ​in the ​DecorImage or SmartLook range of laminate ​finish type and ​Group 2 in ​Natural timber veneers]
* Cewood cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**