Cewood

**HOW TO WRITE UP YOUR SPECIFICATION**

*Please note that some options are available in stock and ready for immediate despatch and are listed below. Other items available on 20+ week lead time.*

* Interior panelling shall be **Cewood** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Thickness Panel: \_\_\_\_mm (15/25/35mm)
* Strand Structure to be \_\_\_\_\_\_\_\_\_\_\_ [please choose a thickness strand option]:
	+ • S — Super Fine, 1 mm (IN STOCK, AVAILABLE FOR IMMEDIATE DESPATCH)
	+ • F — Fine, 1.5 mm
	+ • R — Regular, 3 mm
* Edge Profile to be \_\_\_\_\_\_\_\_\_\_ please choose an edging option:
	+ PO – Panel without Chamfer (IN STOCK, AVAILABLE FOR IMMEDIATE DESPATCH)
	+ P5 – Panel with 5mm chamfer (IN STOCK, AVAILABLE FOR IMMEDIATE DESPATCH)
	+ P11 – Panel with 11mm chamfer
	+ PO-T24 Standard T24 ceiling profile
	+ P0G-T24 Immersed Ceiling Profile
	+ P5G-T24 – Immersed ceiling profile with 5mm chamfer
	+ P5H - Hidden suspended ceiling profile with 5 mm chamfer
	+ P5S - Hidden suspended ceiling profile with overhang and 5 mm chamfer
* Panels to be coloured to be \_\_\_\_\_\_ [Natural or RAL \_\_\_\_\_\_\_ (Insert Code)]
* Panels to be ​Fire Group 1 per BCA ​Specification ​C1.10 clause 4.
* Cewood cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**