DecorZen

**HOW TO WRITE UP YOUR SPECIFICATION**

* Interior panelling shall be **DecorZen** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Profile: \_\_\_\_\_\_\_\_\_\_\_ (Insert artwork name selected)
* Finish: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (Choose from Natural timber veneers, 2 pack poly colours or the range of laminates available)
* Substrate of panels to be \_\_\_ (Choose from: FR MDF / MR MDF / Plywood / OSB Board / Black MDF / Other)
* Joint to be \_\_\_\_\_\_\_\_\_\_\_ [please choose a joint option: (Square / Arrised)]
* Edging to be \_\_\_\_\_\_\_\_\_\_[please choose an edging option: (Matching / Black / N/A)]
* DecorZen panels shall be supplied with DecorSorb Integrated Acoustic Backing.
* Panels to be include DecorInsul behind the panels.
* Decor Systems to supply Black Backing Strips as part of system.
* BioPanel Zap-X to be applied.
* Panels to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4. ​[Note that fire ​groups 1 is ​only available ​in the ​DecorImage or SmartLook range of laminate ​finish type and ​Group 2 in ​Natural timber veneers]
* DecorZen cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**