DecorSlatMaxCreate

**How to write a specification:**

* Interior Slat beams shall be **DecorSlat MaxCreate** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Profile: DST\_\_ (Insert Letter according to profile chosen)
* Finish: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (Choose from solid timbers, 2 pack poly colours or the range of laminates available)
* Backing board to be \_\_\_\_ (Choose from Acoustic panel / Solid backing for decorative purposes or Cross Battens for an open backing
* DecorSlat Max Create beams shall be supplied with DecorSorb Integrated Acoustic Backing.
* Panels to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4. ​[Note that fire ​groups 1 is ​only available ​in the ​DecorImage or SmartLook range of laminate ​finish type and ​Group 2 in ​Natural timber veneers] ​(Contact your project consultant on 1800 835 035 to discuss group 1 fire ratings for solid timber using Fireshield.
* DecorShield to be applied.
* DecorSlat Max Create cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer​’s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**