DecorSlot

**How to write your specification:**

* Panelling shall be **DecorSlot** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Profile: \_\_\_ (Insert profile code required – refer to brochure for available options)
* Finish: \_\_\_\_\_\_ [Raw or Undercoated. (*If perforations are larger than 10mm it is recommended the panels be undercoated to ensure inside of the perforated holes is finished*)]
* DecorSlot panels shall be supplied with DecorSorb Integrated Acoustic Backing.
* Panels to be ​Fire Group 1
* DecorSlot cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Installation: \_\_\_\_\_\_ (Flush / Express / Butt) jointing. Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**