DecorEagle

**How to write your specification:**

* Interior panelling shall be **DecorEagle** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Profile: (Insert profile code required – refer to brochure for available options)
* Finish: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (Custom finishes available or select finish from range of options shown in brochure)
* DecorSorb acoustic IAB backing applied to rear of all panels.
* Decor Systems to supply Black Backing Strips as part of system if applicable.
* BioPanel Zap-X to be applied.
* Panels to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4. ​[Note that fire ​groups 1 is ​only available ​in the ​DecorImage or SmartLook range of laminate ​finish type and ​Group 2 in ​Natural timber veneers] ​(Contact your project consultant on 1800 835 035 to discuss group 1 fire ratings for natural timber veneers using Fireshield.
* DecorEagle cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**