DecorSlat

**How to write specification:**

* Interior Slat panelling shall be **DecorSlat** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Profile: DST\_\_ (Insert Letter according to profile chosen)
* Finish: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (Choose from solid timbers, 2 pack poly colours or the range of laminates available)
* Backing board to be \_\_\_\_ (Choose from Acoustic panel / Solid backing for decorative purposes or Cross Battens for an open backing
* DecorSlat panels shall be supplied with DecorSorb Integrated Acoustic Backing.
* Panels to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4. ​[Note that fire ​groups 1 is ​only available ​in the ​DecorImage or SmartLook range of laminate ​finish type and ​Group 2 in ​Natural timber veneers] ​(Contact your project consultant on 1800 835 035 to discuss group 1 fire ratings for solid timber using Fireshield.
* DecorShield to be applied.
* DecorSlat cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer​’s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**