DecorTone

**HOW TO WRITE UP YOUR SPECIFICATION**

* Interior panelling shall be **DecorTone** by Decor Systems.
* Supplier: Decor Systems Ph: 1800 835 035
* Substrate of panels to be \_\_\_ (Choose from: Solid Timber: Western Red Cedar / Hemlock / Hoop Pine / MR MDF)
* Jointing to be tounge and grooved for seamless fixing
* Panels to be ​Fire Group 3 / ​2 / 1 [delete ​as required] ​per BCA ​Specification ​C1.10 clause 4. ​[Note that fire ​groups 1 is ​only available with the application of Fireshield] ​(Contact your project consultant on 1800 835 035 to discuss group 1 fire ratings
* DecorTone cannot to be substituted unless agreed by Architect and Acoustic Engineer. Panels should be allowed to acclimatise on site for at least five days before installation. Decor Systems certificate # (Contact your Decor Systems project consultant for your individual project number) to be supplied upon completion.
* Panel ​installation to ​be as per ​manufacturer'​s instructions ​and AS/NZS 2785.​ - Installation ​to be done ​by an approved ​ceiling and ​partition ​contractor. ​
* Product ​guarantee to be ​99 years as per Decor Systems guarantee.
* **Please contact Decor Systems for your project specific completion number.**