|  |  |
| --- | --- |
|  |  |
| Property Address  |  |
|  |  |
| CC or CDC Application No.  |  |
|  |  |
| Description of WorkBeing Certified |  |
| I hereby certify that:* All windows where the floor below the window in a bedroom is 2m or more above the surface beneath, and the level of the window opening is less than 1.7m above the floor, have been protected with a device capable of restricting the window opening, or a screen with secure fittings in accordance with Clause 3.9.2.6 of Volume 2 of the BCA 2019. If the lowest part of the opening is within 865mm of the floor level, or there are climbable elements between 150mm and 760mm, the device permanently restricts the window opening.
* All window openings to a room other than a bedroom have been provided with protection where the floor level below the winow is 4m or more above the surface beneath.
* The openable part of the window covered by the above have been provided with a barrier with a height of not less than 865mm above the floor.
* The provided barrier does not permit a 125mm sphere to pass through it and have any horizontal or near horizontal elements between 150mm and 760mm above the floor that faulitate climbing.

I confirm that I am appropriately competent and qualified to certify this element. |
| Details of the PersonMaking the Statement | Name: Email: Phone No.: Licence No.: Company:  |
|  |  |
| Date |  |
|  |  |
| Signature |  |