**SECTION 05 70 00**

**DECORATIVE STAINLESS STEEL FACING MATERIAL**

1. GENERAL
	1. Summary
		1. Section Includes: Decorative stainless steel facing material.
	2. References
		1. ASTM A 480/A 480M - Specification for General Requirements for Flat-Rolled Stainless and Heat-Resisting Steel Plate, Sheet, and Strip.
		2. ASTM E 527 - Practice for Numbering Metals and Alloys (UNS).
	3. Submittals
		1. Submit samples no less than 4" x 4" of decorative stainless steel face material in finish specified.
		2. Manufacturer information:
			1. Provide overview literature describing manufacturer’s overall scope of products and manufacturing capabilities.
			2. Provide URL for manufacturer’s web site; web site must provide access to technical data, images and general product information.
			3. Provide manufacturer’s toll-free telephone number for product support.
	4. Quality Assurance
		1. Manufacturer Qualifications
			1. Minimum 10 years experience in the manufacture of stainless steel sheet goods and fabricated products.
			2. Provide reference list of at least 10 public space projects currently using decorative stainless steel facing materials produced by the manufacturer in the finish specified.
	5. Delivery, Storage and Handling
		1. Deliver material to installation site in manufacturer’s original packaging. Store in a flat, horizontal position. Protect material against abrasion and impacts. Do not stack other materials or equipment on top of stainless steel sheets.
		2. Handle sheets carefully to avoid kinking.
		3. When practical, leave strippable films in place until installation is completed.
2. PRODUCT
	1. Manufacturer
		1. Forms+Surface
		30 Pine Street
		Pittsburgh, PA 15223
		phone: 800-451-0410
		fax: 412-385-4715
		email: sales@forms-surfaces.com
		website: [www.forms-surfaces.com](http://www.forms-surfaces.com/)
		2. Substitutions: not acceptable.
	2. Stainless Steel
		1. Material: Stainless Steel.
		2. Finish: Sandstone, Seastone, Linen, Diamond, Mist, Satin (choose one)
		3. Impression Pattern: Champagne, Chardonnay, Dallas, Denver, Dune, Kalahari (choose one)
		4. Eco-Etch Pattern: City Lights, Current, Dash, Flicker, Glacier, Mica, Reeds, Seagrass, Sequence, Silkworm, Stacks, Stripe, Thatch, Trace (choose one)
		5. Fire rating: Stainless Steel inherently non-combustible and generally considered to be NFPA and IBC Class A fire rated and UBC Class 1 fire rated.
		6. Treatment: Provide Ceramiloc+™ treatment, an invisible, protective treatment that significantly increases the fingerprint resistance and maintenance ease of stainless steel. Patented technology molecularly bonds nano-silica particles to the surface of stainless steel.
3. EXECUTION
	1. Examination
		1. Inspect material to ensure that no damage has occurred prior to installation.
	2. Preparation
		1. Protect adjoining finishes, fixtures and equipment from damage caused by work of this Section.
	3. Installation
		1. Install material according to architect’s drawings.
		2. Ensure that installation complies with all applicable local building codes.
	4. Cleaning and Protection
		1. Remove strippable film. Clean exposed surfaces in accordance with manufacturer’s instructions.
		2. Protect exposed surfaces from damage by subsequent construction.

END OF SECTION