;Diameter##LENGTH##INCHES;Light Source##OTHER##;Color Temperature (K)##OTHER##;Light Distribution##ANGLE##DEGREES;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Wattage##ELECTRICAL_WATTAGE##WATTS;Type Comments##OTHER##;Keynote##OTHER##;z_type_index##OTHER##
Series 600 Non-Illuminated Surface Mount;6.0;Light_Source : None;0;0;0;0;Cyrca Bollard, Series 600, Non-Illuminated,Surface Mount;34 71 00.A1;1
Series 900 Non-Illuminated Surface Mount;9.25;Light_Source : None;0;0;0;0;Cyrca Bollard, Series 900, Non-Illuminated,Surface Mount;34 71 00.A1;2
Series 600 Non-Illuminated Deep Set Mount;6.0;Light_Source : None;0;0;0;0;Cyrca Bollard, Series 600, Non-Illuminated,Deep Set Mount;34 71 00.A1;4
Series 900 Non-Illuminated Deep Set Mount;9.25;Light_Source : None;0;0;0;0;Cyrca Bollard, Series 900, Non-Illuminated,Deep Set Mount;34 71 00.A1;5
Series 600 Non-Illuminated Shallow Mount;6.0;Light_Source : None;0;0;0;0;Cyrca Bollard, Series 600, Non-Illuminated,Shallow Mount;34 71 00.A1;7
Series 900 Non-Illuminated Shallow Mount;9.25;Light_Source : None;0;0;0;0;Cyrca Bollard, Series 900, Non-Illuminated,Shallow Mount;34 71 00.A1;8
Series 600 Illuminated 3000K Surface Mount;6.0;Light_Source : 600, 360deg, 3000K;3000;360;65;30;Cyrca Bollard, Series 600, Illuminated, 3000K, Surface Mount;26 56 00;11
Series 600 Illuminated 4000K Surface Mount;6.0;Light_Source : 600, 360deg, 4000K;4000;360;65;30;Cyrca Bollard, Series 600, Illuminated, 4000K, Surface Mount;26 56 00;13
Series 600 Illuminated 3000K Deep Set Mount;6.0;Light_Source : 600, 360deg, 3000K;3000;360;65;30;Cyrca Bollard, Series 600, Illuminated, 3000K, Deep Set Mount;26 56 00;15
Series 600 Illuminated 4000K Deep Set Mount;6.0;Light_Source : 600, 360deg, 4000K;4000;360;65;30;Cyrca Bollard, Series 600, Illuminated, 4000K, Deep Set Mount;26 56 00;17
Series 600 Illuminated 3000K Shallow Mount;6.0;Light_Source : 600, 360deg, 3000K;3000;360;65;30;Cyrca Bollard, Series 600, Illuminated, 3000K, Shallow Mount;26 56 00;19
Series 600 Illuminated 4000K Shallow Mount;6.0;Light_Source : 600, 360deg, 4000K;4000;360;65;30;Cyrca Bollard, Series 600, Illuminated, 4000K, Shallow Mount;26 56 00;21
Series 900 Illuminated 3000K Surface Mount;9.25;Light_Source : 900, 360deg, 3000K;3000;360;65;30;Cyrca Bollard, Series 900, Illuminated, 3000K, Surface Mount;26 56 00;23
Series 900 Illuminated 4000K Surface Mount;9.25;Light_Source : 900, 360deg, 4000K;4000;360;65;30;Cyrca Bollard, Series 900, Illuminated, 4000K, Surface Mount;26 56 00;25
Series 900 Illuminated 3000K Deep Set Mount;9.25;Light_Source : 900, 360deg, 3000K;3000;360;65;30;Cyrca Bollard, Series 900, Illuminated, 3000K, Deep Set Mount;26 56 00;27
Series 900 Illuminated 4000K Deep Set Mount;9.25;Light_Source : 900, 360deg, 4000K;4000;360;65;30;Cyrca Bollard, Series 900, Illuminated, 4000K, Deep Set Mount;26 56 00;29
Series 900 Illuminated 3000K Shallow Mount;9.25;Light_Source : 900, 360deg, 3000K;3000;360;65;30;Cyrca Bollard, Series 900, Illuminated, 3000K, Shallow Mount;26 56 00;31
Series 900 Illuminated 4000K Shallow Mount;9.25;Light_Source : 900, 360deg, 4000K;4000;360;65;30;Cyrca Bollard, Series 900, Illuminated, 4000K, Shallow Mount;26 56 00;33