If you want to restore SX:ACCESS to the default configuration you need to transfer the default config-file back to the central.

There are two files with different languages. E stands for English.
SMOKE_DEFAULT_E.cfg
SMOKE_DEFAULT.cfg

1. Start the PC-software SIOX Smoke Manager. Installation file can be found in folder "2. Software".

2. Connect to your SX:ACCESS by typing its IP-address. Click "Connect". A picture of the central should pop up.

3. In the menu, go to "PREFERENCES" and then expand "ADVANCED.." on the bottom of the page.

4. Next to "Write CFG file to siox unit", click "Open".

5. In the new popup, click "Central unit" and then "Select file".

6. Browse for the config-file. E.g. "SMOKE_DEFAULT.cfg". Click "Open".

7. Then click "Upload"

8. The file is now transfered.

9. Done.