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Range at a Glance
	Model
	Type
	Width
	Tank
	Productivity / Speed

	VSD 43/4-Ep
	Compact scrubber (corded)
	430 mm
	4 / 5 L
	1200 m²/h

	VSD 43/4-Bp
	Compact scrubber (battery)
	430 mm
	4 / 5 L
	1200 m²/h

	VSD 30/40-Ep
	Compact scrubber (corded)
	400 mm
	30 / 40 L
	1700 m²/h

	VSD 46/40-Ep
	Walk-behind scrubber (corded)
	460 mm
	40 / 40 L
	1900 m²/h

	VSD 46/40-Bp
	Walk-behind scrubber (battery)
	460 mm
	40 / 45 L
	1900 m²/h

	VSD 50/60-Ep
	Walk-behind scrubber (corded)
	530 mm
	50 / 60 L
	2100 m²/h

	VSD 50/60-Bp
	Walk-behind scrubber (battery)
	530 mm
	50 / 60 L
	2100 m²/h

	VSD 43/150 (1.5 HP)
	Single-disc machine
	430 mm
	10 L
	150–160 RPM

	VSD 43/150 (2 HP)
	Single-disc machine
	430 mm
	10 L
	160 RPM

	VDP 1500
	Single-disc polisher
	508 mm
	—
	1500 RPM


Ep = electric powered (corded)   ·   Bp = battery powered. Tank shown as solution / recovery capacity where applicable.


1.  VOOT VSD 43/4-Ep
Compact Scrubber Drier (Corded)
Description
A corded compact scrubber drier delivering exceptional performance in a lightweight format. Like its battery-operated counterpart, it achieves a 97% dirt-removal rate, greatly enhancing hygiene while leaving floors dry and safe immediately after use to reduce slip hazards. Its eco-friendly design minimizes water and chemical use without sacrificing cleaning power, and simple parts replacement keeps maintenance easy. As a corded unit it runs continuously with no recharge downtime, making it a fast, safe and effective replacement for manual mopping.
Key Features
1. Corded for Continuous Operation: No recharge time — uninterrupted cleaning.
1. Efficient Water & Chemical Usage: Eco-friendly with strong cleaning power.
1. High-Speed, Edge-to-Edge Cleaning: Reaches edges and under obstacles.
1. Slip-Free Results: Immediate dry finish ideal for public spaces.
1. Simple Parts Replacement: Easy, low-effort maintenance.
Technical Details
	Make
	VOOT

	Voltage
	220–240 V / 50 Hz

	Power Source
	Electric (corded)

	Cleaning Width
	430 mm

	Squeegee Width
	450 mm

	Solution Tank
	4 L

	Recovery Tank
	5 L

	Efficiency
	1200 m²/h

	Brush Pressure
	8 Kg

	Suction Motor
	200 W

	Brush Motor
	150 W

	Cleaning Efficiency
	Over 97%

	Drying Time
	Immediate

	Noise Level
	< 60 dBA

	Weight
	17 Kg

	Dimensions (L × W × H)
	568 × 465 × 1215 mm


Application Areas
1. Hospitals and clinics
1. Supermarkets and shopping centres
1. Schools and universities
1. Corporate offices
1. Gyms and leisure venues


2.  VOOT VSD 43/4-Bp
Compact Scrubber Drier (Battery)
Description
A battery-powered compact scrubber drier known for outstanding cleaning efficiency and safety. It achieves a 97% dirt-removal rate — far superior to traditional mopping — and leaves floors dry, clean and slip-resistant. Operating with significantly less water and energy, it supports sustainable cleaning, while its high-capacity lithium battery and compact design make it perfect for confined areas and cleaning under obstacles, eliminating the need for manual follow-up.
Key Features
1. Proven 97%+ Dirt Removal: Superior hygiene versus mopping.
1. Lithium Battery: Extended runtime with fast charging.
1. Non-Slip, Dry Finish: Enhanced safety immediately after cleaning.
1. Saves up to 75% Water: Compared to traditional methods.
1. Compact and Maneuverable: Perfect for edges and under furniture.
Technical Details
	Make
	VOOT

	Voltage
	220–240 V / 50 Hz (charger)

	Power Source
	Lithium-ion battery

	Cleaning Width
	430 mm

	Squeegee Width
	450 mm

	Solution Tank
	4 L

	Recovery Tank
	5 L

	Efficiency
	1200 m²/h

	Brush Pressure
	8 Kg

	Suction Motor
	200 W

	Brush Motor
	150 W

	Dirt Removal Efficiency
	Over 97%

	Water Saving
	75% less water usage

	Noise Level
	< 60 dBA

	Weight
	17 Kg

	Dimensions (L × W × H)
	568 × 465 × 1215 mm


Application Areas
1. Retail spaces
1. Healthcare environments
1. Educational institutions
1. Commercial buildings
1. Industrial and logistics centres


3.  VOOT VSD 30/40-Ep
Compact Scrubber Drier (Corded)
Description
A compact, walk-behind scrubber drier built for professional cleaning of commercial and industrial spaces. Designed for high-traffic areas, it offers a cleaning capacity of 1,700 m²/h with a 40-litre recovery tank. Its ergonomic design ensures superior maneuverability in tight areas while maintaining clear visibility of the surface, and its disc brush and squeegee system provide deep scrubbing and quick drying for clean, slip-free floors. Durable construction and a 270° adjustable handle balance high performance with affordability.
Key Features
1. Compact Design: 40-litre tank capacity in a maneuverable body.
1. Disc Brush & Squeegee: Effective scrubbing and quick drying.
1. 270° Adjustable Handle: Ergonomic comfort for the operator.
1. Exceptional Maneuverability: Navigates confined spaces with ease.
1. Clear Visibility & Simple Operation: Easy to learn and use.
Technical Details
	Make
	VOOT

	Voltage
	230 V / 50 Hz

	Cable Length
	15 m

	Cleaning Path
	400 mm

	Squeegee Width
	580 mm

	Brush Diameter
	400 mm

	Fresh Water Tank
	30 L

	Dirty Water Tank
	40 L

	Vacuum Motor
	500 W

	Brush Motor
	400 W

	Productivity
	1700 m²/h

	Handle Adjustment
	270°

	Weight
	86 Kg

	Dimensions (L × W × H)
	910 × 510 × 720 mm


Application Areas
1. Hospitals and healthcare facilities
1. Schools and educational institutions
1. Warehouses and industrial sites
1. Shopping centres and retail stores
1. Airports and transport hubs


4.  VOOT VSD 46/40-Ep
Walk-Behind Auto Scrubber (Corded)
Description
The mains-powered twin of the 46/40-Bp, providing the same 460 mm scrubbing width, 40-litre tank, advanced disc brush and ergonomic design, but powered via a cable for non-stop operation. Ideal for smaller or medium spaces needing continuous cleaning, it eliminates battery-charging downtime. Durable and easy to use, it offers exceptional visibility and maneuverability backed by robust construction for long-term use.
Key Features
1. Corded (20 m Cable): Non-stop cleaning without recharge.
1. Compact yet Powerful: 1900 m²/h cleaning capacity.
1. Low-Profile Design: Ergonomic controls and clear line of sight.
1. Integrated Disc Brush & Squeegee: Efficient scrubbing and water pick-up.
1. Built for High-Traffic: Suited to medium-sized environments.
Technical Details
	Make
	VOOT

	Voltage
	230 V / 50 Hz

	Cable Length
	15 m

	Cleaning Path
	460 mm

	Squeegee Width
	780 mm

	Brush Diameter
	460 mm

	Fresh Water Tank
	40 L

	Dirty Water Tank
	40 L

	Vacuum Motor
	500 W

	Brush Motor
	550 W

	Productivity
	1900 m²/h

	Weight
	60 Kg

	Dimensions (L × W × H)
	1080 × 500 × 1075 mm


Application Areas
1. Hospitals
1. Educational institutions
1. Manufacturing floors
1. Department stores
1. Logistics warehouses


5.  VOOT VSD 46/40-Bp
Walk-Behind Auto Scrubber (Battery)
Description
A battery-operated walk-behind auto scrubber designed for high-traffic environments, offering up to 3–4 hours of runtime with a compact 460 mm scrubbing width and 40-litre tanks. A magnetic brush/squeegee system and disc brush technology remove industrial residues with minimal effort at a cleaning capacity of 1900 m²/h — ideal for areas without easy access to power outlets. Intuitive controls, an ergonomic handle and a clear line-of-sight design reduce operator fatigue and training time.
Key Features
1. Cordless Operation: Up to 4-hour runtime.
1. Compact yet Powerful: 460 mm cleaning width.
1. Magnetic Brush & Squeegee System: Tool-free changes and easy handling.
1. 40-Litre Dual Tanks: Extended cleaning between refills.
1. Intuitive Controls: Ergonomic layout reduces fatigue.
Technical Details
	Make
	VOOT

	Cleaning Path
	460 mm

	Squeegee Width
	780 mm

	Battery
	12 V / 100 Ah × 2

	Charger
	220 V 50 Hz / 110 V 60 Hz

	Solution / Recovery Tank
	40 / 45 L

	Vacuum Motor
	500 W

	Brush Motor
	400 W

	Productivity
	1900 m²/h

	Brush Type
	Magnetic disc brush

	Working Time
	3–4 hours

	Charging Time
	6–8 hours

	Noise
	< 60 dBA

	Weight
	120 Kg

	Dimensions (L × W × H)
	1080 × 500 × 1075 mm


Application Areas
1. Hospitals
1. Warehouses
1. Shopping malls
1. Schools and universities
1. Industrial factories


6.  VOOT VSD 50/60-Ep
Walk-Behind Auto Scrubber (Corded)
Description
A powerful, mains-operated walk-behind scrubber designed for medium to large-scale cleaning, delivering a theoretical performance of 2,100 m²/h. It shares the same platform as the battery version but is powered via a 20-metre cable, eliminating charging downtime for environments with continuous cleaning needs. Its advanced disc brush system with a long-life bristle splash guard delivers consistent, streak-free results, and with a 60-litre tank and wide working width it is both efficient and cost-effective.
Key Features
1. Continuous Mains Power: 20-metre cable for uninterrupted cleaning.
1. Durable Brush System: Extended splash-guard life for consistency.
1. Wide Cleaning Width: Fast, thorough coverage.
1. Ergonomic Controls: Clear operator view and easy handling.
1. Affordable & Effective: Cost-effective for high-traffic zones.
Technical Details
	Make
	VOOT

	Voltage
	230 V

	Cleaning Path
	530 mm

	Squeegee Width
	780 mm

	Brush Diameter
	530 mm

	Fresh Water Tank
	50 L

	Dirty Water Tank
	60 L

	Vacuum Motor
	500 W

	Brush Motor
	550 W

	Productivity
	2100 m²/h

	Weight
	130 Kg

	Dimensions (L × W × H)
	1270 × 550 × 1090 mm


Application Areas
1. Educational campuses
1. Clinics and hospitals
1. Production facilities
1. Retail and showroom floors
1. Industrial sites with steady power access


7.  VOOT VSD 50/60-Bp
Walk-Behind Auto Scrubber (Battery)
Description
An advanced, battery-powered walk-behind auto scrubber drier for medium to large commercial and industrial areas. A powerful dual-battery system provides up to 3–5 hours of runtime alongside a 60-litre solution/recovery tank, suiting extended cleaning sessions. With a theoretical cleaning capacity of up to 2,100 m²/h and a wide scrubbing path, it offers superior productivity, while its integrated disc brush uses a bristle splash guard up to 10× more durable than traditional guards. Compact yet sturdy construction ensures maximum mobility, reliability and efficiency.
Key Features
1. Long Battery Runtime: 3–5 hrs with dual 12 V batteries.
1. Large 60-Litre Tank: Fewer refills, longer sessions.
1. Bristle Splash Guard: Enhances brush durability up to 10×.
1. Wide Working Width: 530 mm path with 780 mm squeegee.
1. Ergonomic Handle: EASY-operation control panel.
Technical Details
	Make
	VOOT

	Battery
	12 V 150 Ah × 2

	Cleaning Path
	530 mm

	Squeegee Width
	780 mm

	Brush Diameter
	530 mm

	Fresh Water Tank
	50 L

	Dirty Water Tank
	60 L

	Vacuum Motor
	550 W

	Brush Motor
	550 W

	Productivity
	2100 m²/h

	Weight
	220 Kg

	Dimensions (L × W × H)
	1270 × 550 × 1090 mm


Application Areas
1. Hospitals and healthcare centres
1. Warehouses and distribution hubs
1. Schools and universities
1. Supermarkets and shopping malls
1. Manufacturing and production floors


8.  VOOT VSD 43/150 (1.5 HP)
Single Disc Machine
Description
A robust single-disc floor machine optimized for scrubbing, polishing, stripping and buffing. Its maintenance-free planetary gear system delivers high torque with minimal wear, outperforming belt-driven alternatives. Ideal for industrial and commercial use, it offers quiet operation, excellent balance and ergonomic handling. A rotary water control system allows precise moisture management during cleaning, while a splash-proof IPX4 design ensures safe operation in wet environments. A durable, corrosion-resistant frame and large wheels make it suited to demanding, high-traffic spaces.
Key Features
1. 1.5 HP Motor: Strong, reliable cleaning power.
1. Maintenance-Free Planetary Gear: Reduced upkeep with metal gears.
1. Splash-Proof IPX4: Safe in wet environments.
1. Rotary Water Control: Precise moisture application.
1. Ergonomic & Quiet: Excellent balance for comfortable use.
Technical Details
	Make
	VOOT

	Voltage
	230 V / 50 Hz

	Working Width
	430 mm (17 in)

	Water Tank Capacity
	10 L

	Motor Power
	1.5 HP

	Brush / Disc Speed
	150–160 RPM

	Gear System
	Planetary (metal gears)

	Ingress Protection
	IPX4

	Cable Length
	10–15 m

	Weight
	48 Kg

	Dimensions (L × B × H)
	590 × 430 × 1180 mm


Application Areas
1. Factories and warehouses
1. Hospitals and clinics
1. Schools and universities
1. Hotels and resorts
1. Retail stores and malls
1. Transport hubs


9.  VOOT VSD 43/150 (2 HP)
Single Disc Machine
Description
The 2 HP variant offers increased power over the 1.5 HP model, providing unmatched performance for deep cleaning and restoration. It keeps the same core features — planetary gear transmission, IPX4 splash-proof body and ergonomic controls — but boosts output to meet tougher industrial challenges. Its rotary water control, enhanced torque and compatibility with various brushes and pads make it a go-to for stripping, buffing and polishing, while a push-button storage handle and robust frame suit both high-volume and space-restricted facilities.
Key Features
1. Powerful 2 HP Motor: Handles tougher jobs with ease.
1. Gear-Driven (Not Belt): Longevity and higher torque.
1. Ergonomic Push-Handle: Foldable design for storage.
1. Industrial-Grade Stripping/Polishing: Built for demanding tasks.
1. Quiet & Splash-Proof: IPX4-rated for indoor use.
Technical Details
	Make
	VOOT

	Voltage
	230 V / 50 Hz

	Working Width
	430 mm (17 in)

	Water Tank Capacity
	10 L

	Motor Power
	2 HP

	Brush Speed
	160 RPM

	Gear System
	Planetary (metal gears)

	Ingress Protection
	IPX4

	Cable Length
	12 m

	Frame
	Heavy-duty, corrosion-resistant

	Weight
	48 Kg

	Dimensions (L × B × H)
	590 × 430 × 1180 mm


Application Areas
1. Manufacturing plants
1. Logistics centres
1. Large retail chains
1. Public transport stations
1. Cruise ships and marine decks


10.  VOOT VDP 1500
Single Disc Floor Polishing Machine
Description
A high-performance single-disc floor polishing machine for industrial, commercial and institutional use. A powerful 1100 W (1.5 HP) motor spinning at 1500 RPM delivers professional-grade polishing and cleaning on marble, granite, vinyl, hardwood and terrazzo. Robust construction with an ergonomic design ensures long-lasting performance and easy operation, while quiet operation (under 60 dB) and excellent balance suit noise-sensitive environments like hospitals and offices. An IPX4 splash-proof rating, eco-conscious energy use, included brushes and pads, and wide voltage compatibility make it a versatile, reliable choice worldwide.
Key Features
1. High-Speed Polishing: 1500 RPM for a glossy, spotless finish.
1. Robust 1100 W Motor (1.5 HP): Powerful for heavy-duty polishing and cleaning.
1. Low Noise & Balanced Design: Smooth, quiet operation below 60 dB.
1. Versatile Accessories: Polishing pads, brushes and attachments included.
1. Eco-Friendly & Safe: IPX4 water resistance and overload protection.
Technical Details
	Make
	VOOT

	Voltage
	220–240 V / 50 Hz

	Working Width
	508 mm

	Motor Power
	1100 W (1.5 HP)

	Rotational Speed
	1500 RPM

	Current Consumption
	5 Amp

	Noise Level
	Below 60 dB

	Ingress Protection
	IPX4 (splash-proof)

	Cable Length
	10–15 m

	Frame Material
	Corrosion-resistant heavy-duty metal

	Accessories Included
	Pads, brushes

	Weight
	53 Kg

	Dimensions (L × B × H)
	500 × 330 × 630 mm


Application Areas
1. Commercial Facilities: Offices, malls, hotels and retail outlets.
1. Hospitality & Leisure: Resorts, banquet halls, fitness centres and venues.
1. Educational Institutions: Schools and universities in high-traffic areas.
1. Healthcare & Pharmaceuticals: Clinics and hospitals needing safe, polished floors.
1. Industrial Environments: Factories, warehouses and logistics hubs.
1. Retail & Showrooms: Luxury outlets, dealerships and supermarkets.
1. Transportation Hubs: Airports, railway and bus terminals.
1. Residential Complexes: Premium apartments, condominiums and homes.
