|  |  |
| --- | --- |
|  |  |
| Property Address  |  |
|  |  |
| CC or CDC Application No.  |  |
|  |  |
| Description of WorkBeing Certified |  |
| I hereby certify that:Wall to BoundaryThat the walls within 900mm of the property boundary have been constructed with a Fire Resistance Level (FRL) of not less than 60/60/60 as required by Part 3.7.2 *“Construction of External Walls”* of Volume 2 of the BCA 2019.Separation of Dwellings – Wall to Wall (same lot) That the walls within 1.8m of another dwelling within the property lot have been constructed with a Fire Resistance Level (FRL) of not less than 60/60/60 as required by Part 3.7.2 “Construction of External Walls” of Volume Two of the BCA 2019.The material specifications, if not approved or have changed from the approved Construction Certificate specifications, have been enclosed. I confirm I am appropriately competent and qualified to certify this element. |
| Details of the PersonMaking the Statement | Name: Email: Phone No.: Licence No.: Company:  |
|  |  |
| Date |  |
|  |  |
| Signature |  |