**NCC 2022 – Volume Two (Including any amendment adoptions)**

|  |  |
| --- | --- |
|  |  |
| Property Address |  |
|  |  |
| CC or CDC  Application No. |  |
|  |  |
| Description of Work  Being Certified |  |
| I hereby certify that:  The constructed separating walls have a Fire Resistance Level (FRL) of not less than 60/60/60 as required by Part 9.3 *“Fire Protection of Separating Walls and Floors”* of Volume 2 of the BCA 2022 – Housing Provisions.  In addition, the separating wall achieves the weighted sound reduction index with spectrum adaptation term (Rw + Ctr) and impact sound resistance for separating walls between Class 1 building (dwelling) and any servicing that passes through a separating wall between Class 1 buildings as required by Part 10.7 *“Sound insulation”* and Part 9.3 “*Fire protection of separating walls and floors”* of Volume 2 of the BCA 2022 – Housing Provisions.  Where the development includes horizontal projections within the Separating wall system, they are constructed in accordance with Clause 9.3.4 *“Horizontal projections”* of Volume 2 of the BCA 2022 – Housing Provisions.  The material specifications, if not approved or have changed from the approved Construction/CDC Certificate specifications, have been enclosed. I confirm I am appropriately competent and qualified to certify this element. | |
| Details of the Person  Making the Statement | Name:  Email:  Phone No.:  Licence No.:  Company: |
|  |  |
| Date |  |
|  |  |
| Signature |  |