|  |  |
| --- | --- |
|  |  |
| Property Address |  |
|  |  |
| CC or CDC  Application No. |  |
|  |  |
| Description of Work  Being Certified |  |
| I hereby certify that:  The constructed separating walls have a Fire Resistance Level (FRL) of not less than 60/60/60 as required by Clause 3.7.3.2 *“Separating Walls”* of Volume 2 of the BCA 2019.  In addition, the separating wall achieves the weighted sound reduction index with spectrum adaptation term (Rw + Ctr) and impact sound resistance for separating walls between Class 1 building (dwelling) and any servicing that passes through a separating wall between Class 1 buildings as required by Part 3.8.6 *“Sound insulation”* and Part 3.7.3 “*Fire protection of separating walls and floors”* of Volume 2 of the BCA 2019.  The material specifications, if not approved or have changed from the approved Construction/CDC Certificate specifications, have been enclosed. I confirm I am appropriately competent and qualified to certify this element. | |
| Details of the Person  Making the Statement | Name:  Email:  Phone No.:  Licence No.:  Company: |
|  |  |
| Date |  |
|  |  |
| Signature |  |